**TWO-SECTION REACH-IN REFRIGERATOR**

Furnish one (1) **Two-Section Reach-In Refrigerator**, Model **HRPS2HC-1HS** as manufactured by **Beverage Air**. Unit shall be equipped with the following standard features:

* Cabinet dimensions to be 52”W x 33.5”D x 85”H overall.
* Cabinet front, ends, interior and doors constructed of heavy gauge, polished stainless steel
* Full electronic controls
* One piece front grille
* LED interior lighting
* Foamed-in-place polyurethane foam insulation throughout the cabinet to insure energy efficiency
* Solid Half Doors
* Doors shall be equipped with one-piece, snap-in magnetic door gasket.
* Doors shall be equipped with self-closing cam-lift hinges having a hold-open feature at 120⁰ to facilitate loading.
* Door locks
* Anti-microbial door handles
* Heavy-duty epoxy coated wire shelves
* Uses environmentally friendly, energy efficient R290 refrigerant and meets all regulatory requirements for CARB, SNAP, DOE and more
* Hot gas condensate evaporator
* Variable speed fan
* Adaptive defrost system
* Epoxy coated evaporator coil
* Maintains product temperatures between 36°F and 38°F

Provide unit with the following accessory features:

* Full complement of stainless steel universal tray slides on 4” centers
* 6” legs in lieu of standard casters
* Door hinging to be verified by Owner.

Utility Requirements:

* Electrical: 115V/60/1Ph, 6.0 amps, 5-15P (8’ cord with plug provided)

Warranty:

* 3 Years Parts and Labor Warranty
* 7 Years Compressor Warranty

Additional requirements:

* Alternates must be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver, uncrate, set in place, level and remove crating.