**BLAST CHILLER**

Provide one (1) **Reach-In Blast Chiller**, Self-Contained, Model **WBC-75** as manufactured by **Beverage Air**. Unit shall be furnished with all standard features as follows:

* Overall dimensions to be 35.5”W x 36”D x 77-1/2”H with casters.
* Cabinet front, sides, door and interior constructed of heavy gauge polished stainless steel
* High density, environmentally friendly 3” insulation throughout
* Flush-mounted, self-closing door with easy-to-replace magnetic balloon gasket
* Door heater standard to prevent condensation from forming on cabinet front
* Two operational functions: Blast chilling processing refrigerator and +38°F storage refrigerator
* 1-2-3 microprocessor control panel with blast chill cycle controlled automatically by either a food probe or digital timer
* Two (2) preset chill times: 90 minutes or 240 minutes
* Soft chill and hard chill options
* Three (3) food probes with digital temperature indication
* Continuous blast feature
* Cabinet temperature digital display and food temperature digital display
* Defrost mode indicator
* Standby, blast chill cycle and cancel buttons
* Diagnostic troubleshooting capability
* Seven (7) day temperature recorder with printout on demand
* Front-breathing design for zero clearance installation
* Complies with FDA, NSF7 and HACCP guidelines
* Twelve (12) pairs tray slides standard
* Chilling capacity in 90 minutes shall be 75 lbs (160°F to 38°F)
* Heavy duty swivel casters with brakes on front
* No drain required

Electrical requirements:

* 208V/60/1Ph, 15.0 amps, 1-1/2 HP
* Provide plug as required

Warranty:

* 3 Years Parts and Labor
* 5 Year Compressor Warranty

Additional requirements:

* Eligible bidder must visit the installation site.
* Alternates must be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver, uncrate, set in place, level and remove crating.
* Final connections by Others.