**HEATED HOLDING AND PROOFING CABINET**

Provide one (1) each **Insulated Heated Holding and Proofing Cabinet**, Model **HL4-18** as manufactured by **Carter-Hoffmann**. Furnish with the following standard features:

* Overall dimensions to be 26.5”W x 31.5”D x 70.5”H including casters.
* Welded and riveted double wall, insulated cabinet construction with cabinet welded to base.
* All aluminum interior and exterior double wall, insulated construction; .063 aluminum exterior with 2V finish. Base frame: .125 natural aluminum.
* 5” diameter casters with rubber tread. Four swivel casters, two fitted with brakes.
* Single panel tempered glass door set in extruded aluminum frame. Field reversible. Drip trough at base of door. High temperature santoprene gasket mounted to door.
* Full width aluminum drip trough with ½” diameter drain located in center, located at base of cabinet. Includes plastic catch pan.
* Adjustable edge mount door hinges with chrome plate finish.
* Heavy duty edge mount door latch with magnetic catch.
* Universal wire tray slides at fixed spacing of 3”. Assemblies removable.
* Capacity for (18) 18” x 26” sheet pans or (36) 12” x 20” steam pans.
* Digital thermometer with remote sensing bulb and sensing bulb protector. Displays temperature in one degree increments.
* Dial type controls. One dial for heat and one dial for humidity level.
* Bottom mounted stainless steel water reservoir is part of heater assembly. Element mounted below pan to provide active humidification. Manual fill. Capacity 2.5 quarts.
* Bottom mounted heater with one 1700 watt coiled incoloy-sheathed heating element. High impedence protected fan motor. Water reservoir with 350 watt element affixed to bottom. Blower fan circulates air and humidity. Full range thermostat and on/off switch with power indicating light. Separate dial controls for heat and humidity.

Electrical requirements:

* 120V/60Hz/1Ph, 2100 watts, 17.5 amps, NEMA 5-20P

Warranty:

* Three Year Parts and Labor Warranty