**HEATED HOLDING AND PROOFING CABINET**

Provide one (1) each **Insulated Heated Holding and Proofing Cabinet**, Model **HL9-18** as manufactured by **Carter-Hoffmann**. Furnish with the following standard features:

* Overall dimensions to be 28”W x 33”D x 76.5”H including casters.
* Completely welded cabinet construction with outer cabinet welded to base. All seams turned in to eliminate raw edges.
* All stainless steel cabinet construction; 20 gauge polished exterior and 18 gauge interior.
* Base frame: 12 gauge stainless steel full depth caster bolsters with 12 gauge stainless steel perimeter supports welded to bolsters.
* 2” thick high density continuous wrap-around type fiberglass insulation.
* 5” diameter casters with rubber tread. Four swivel casters, two fitted with brakes.
* Welded double panel stainless steel door; 20 gauge polished stainless steel exterior and 20 gauge interior. Filled with 2” thick high density fiberglass insulation. Removable stainless steel drip trough at base of door. High temperature Teflon gasket mounted to cabinet.
* Adjustable edge mount door hinges with chrome plate finish.
* Heavy duty edge mount door latch with magnetic catch.
* Four recessed pull grips on sides of cabinet.
* Removable 18 gauge stainless steel. Removable 16 gauge stainless steel universal slides, fully adjustable at 1-1/2” spacing. Standard spacing at 3” centers.
* Capacity for (18) 18” x 26” sheet pans or (36) 12” x 20” steam pans.
* Dial thermometer with remote sensing bulb and sensing bulb protector.
* Dial type controls. One dial for heat and one dial for humidity level.
* Water bath slides out for manual filling. Clear amber color high temperature polycarbonate pan allows for viewing the water level. Slides out for easy filling and removal. 5.7 quart capacity.
* Top mounted heater with one 1000 watt coiled incoloy-sheathed heating element. High impedence protected fan motor. Water reservoir with immersed 1000 watt heating element. Blower fan circulates air and humidity. Extra large surface area to quickly recover humidity level. Full range thermostat and on/off switch with power indicating light.

Electrical requirements:

* 120V/60Hz/1Ph, 2100 watts, 17.5 amps, NEMA 5-20P

Warranty:

* Three Year Parts and Labor Warranty