**30 GALLON GAS TILTING SKILLET**

Provide one (1) **30 Gallon Gas Tilting Skillet**, Model **GLTS-30** as manufactured by **Crown**. Furnish unit with all standard features and equipment as follows:

* Overall dimensions to be 36”W x 39.5”D x 40.25”H.
* Spring assisted, stainless steel cover, with full width handle, no-drip condensate guide and vent port with swing cover.
* Pan shall have a sloped front and be front hinged for easy tilting pour control and shall come complete with a removable pour lip strainer.
* Pan shall be formed from 10 gauge stainless steel with a #4 finish exterior and a polished interior with coved corners for easy cleaning.
* Cooking surface shall be 5/8” thick stainless steel clad plate ensuring even heat distribution over entire cooking surface.
* The pan shall be mounted on a heavy duty welded frame with stainless steel exterior supported by an all welded 1-5/8” stainless steel pipe frame with adjustable bullet feet and rear legs fitted with flange adjustable feet for securing to the floor.
* Controls shall include a ON/OFF power switch, solid state thermostat with OFF position and a range of 100⁰F - 450⁰F, a thermostat indicator light, an ignition indicator light, pan tilt switch that shuts elements off if tilted more than 5⁰, and high temperature cut-off set at 536⁰F.
* Tilting shall be controlled by an electric motor driven ball drive actuator for smooth and precise tilting action.

Furnish unit with accessory features and equipment as follows:

* GMS-30 Etched gallon markings
* TVT-2BP 2” draw-off with strainer
* SF-12 Single pantry faucet with swing spout
* 3” Stainless steel faucet plumbing enclosure

Utility requirements:

* Gas: Gas type to be verified by Owner.
* Electrical: 115V/60/1Ph, 4.0 amps, NEMA 5-15P for controls
* Cold Water: 3/8” O.D. tubing to faucet

Warranty:

* One Year Parts and Labor

Additional requirements:

* Eligible bidder must visit the installation site.
* Alternates must be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver, uncrate, set in place, level and remove crating.
* Final connections by Others.