**DOOR TYPE DISHWASHING MACHINE**

Provide one (1) **High-Temperature** **Door Type Dishwashing Machine,** Model **MD2000HT** as manufactured by **Moyer Diebel**. Unit shall be furnished with all standard features as follows:

* Overall dimensions to be 31.9”W x 28.5”D x 63.8”H with stainless steel adjustable legs.
* Convertible from straight to corner operation in the field
* Built-in booster configured for 40° and 70° rise
* Capacity for 55 racks per hour based upon 60 second cycle
* Water usage of .90 gallons of water per cycle, with water being replenished by final rinse for less water and detergent usage
* Interchangeable stainless steel upper and lower wash rinse arms
* Door safety switch
* Door activated start
* Rinse Sentry
* Detergent chemical connection
* Vent fan control
* Automatic drain valve
* Complete with two (2) 20” x 20” racks, one peg type and one flat

Furnish with the following optional accessories:

* Drain Water Tempering Kit

Utility requirements:

* Electrical: 208/240V; 1/3 phase (field convertible), 1 HP, 13 Kw
* Water: ¾” NPT HW, 110° - 140°, Flow pressure 20-22 psi
* Drain: 2” OD connection gravity drain, 15 GPM max flow
* Exhaust: 350 CFM hood required

Warranty:

* One Year Parts and Labor

Additional requirements:

* Eligible bidder must visit the installation site.
* Alternates must be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver, uncrate, set in place, level and remove crating.
* Final connections by Others.