**HOOD TYPE DISHWASHING/POTWASHING MACHINE**

Provide one (1) **High-Temperature** **Hood Type Dishwashing/Potwashing Machine,** Model **MDHHD** as manufactured by **Moyer Diebel**. Unit shall be furnished with all standard features as follows:

* Overall dimensions to be 34”W x 31.5”D x 69”H with stainless steel adjustable legs.
* Dual NSF listed as both a dishwasher and potwasher
* Convertible from straight to corner operation in the field
* HMI – Operator Touch Screen Interface
* Sleep Mode – all internal heaters shut off after 4 hours idle
* Built-in booster configured to ensure 180° rinse
* Rise Sentry – ensures 180° final rinse
* Auto Start – starts unit when hood is closed
* High efficiency 2 HP pump
* Self-draining pump
* Automatic tank fill
* Automatic drain valve – drains wash tank when power is off
* Mounted Pressure Reducing Valve (PRV)
* 4 selectable cycles
* Vent fan control
* Factory Authorized Startup

Furnish with the following optional accessories:

* Built-in detergent and rinse aid pumps
* Peg Rack
* Flat Rack
* Sheet Pan Rack

Utility requirements:

* Electrical: Voltage/Phase to be verified by Owner, 2 HP, 13 Kw
* Water: ¾” NPT HW, 110° - 140°, Flow pressure 20-22 psi
* Drain: 1.5” OD connection; 15 GPM max flow

Warranty:

* One Year Parts and Labor

Additional requirements:

* Eligible bidder must visit the installation site.
* Alternates must be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver, uncrate, set in place, level and remove crating.
* Final connections by Others.