**DOUBLE ELECTRIC CONVECTION OVEN**

Furnish one (1) **Double Electric Convection Oven**, Model **EB/20SC** as manufactured by **Southbend**. Unit shall be equipped with standard features as follows:

* Overall dimensions to be 38”W x 44”D x 64”H.
* Stainless steel front, top, sides and rear jacket.
* 6” high stainless steel legs.
* 60/40 dependent doors with windows. Stainless steel construction, heavy-duty welded steel frame and 5/8” diameter full-length hinge pin. Heavy duty stainless steel door seals and handle.
* Coved, fastener-free porcelain enamel oven interior
* Oven interior lights
* Soft Air, 2-speed (1710/1120 rpm), 1/2 HP fan motor. Forced cool down fan mode.
* 140⁰F to 500⁰F solid state thermostat and 60-minute mechanical timer.
* Oven “ready” light shall cycle with burners
* Control panel located away from heat zone. Removable panel shall open downward for ease of service.
* Unit shall be 100% serviceable from the front.
* Heavy-duty removable wire rack guides spaced on 1-5/8” centers for 11 rack positions. 5 chrome wire racks shall be provided.
* Plug-in/Plug-out control panel for easy service

Utility requirements (per deck):

* Electrical: 11kW (Voltage and Phase to be verified by Owner prior to ordering)

Warranty:

* Three Year Parts and Labor Warranty
* Five Year Door Warranty

Additional requirements:

* Eligible bidder must visit the installation site.
* Alternates must be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver, uncrate, set in place, level and remove crating.
* Final connections by Others.