**TWO BURNER RANGE**

Provide one (1) **Two Burner Range with Cabinet Base**, Model **P16C-X** as manufactured by **Southbend**. Unit shall be provided with all standard features as follows:

* Overall dimensions to be 16”W x 37-1/2”D x 36”H, including 6” legs.
* Front, sides, rear and exterior bottom constructed of #3 polished 430 and 304 stainless steel.
* Two ***Signature*** Pyromax 45,000 BTU patented clog-free burners
* Removable, welded steel top grate
* Removable stainless steel drip tray
* Fully-insulated lining and burner box
* Stainless steel cabinet base with removable hinged door

Furnish with the following accessory features:

* 5” high flue riser with stainless steel front and sides
* 1” Rear Gas Connection with pressure regulator
* Front manifolds to be capped and covered with stainless steel trim plates.

Utility requirements:

* Gas: 90,000 BTU (Gas type to be verified by Owner)

Warranty:

* Two Years Parts and Labor
* Lifetime Burner Warranty

Additional requirements:

* Alternates need to be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver, uncrate, set in place, level and remove crating.
* Final connections by others.