**10-QUART PLANETARY MIXER**

Provide one (1) **10-Quart Planetary Mixer**, Model **BTF010** as manufactured by **Doyon**. Furnish with standard features as follows:

* Overall dimensions to be 16.5”W x 23” x 33”H
* 20 speeds – no need to stop mixer to change speeds
* Digital control with 7 programmable speed and time settings
* Emergency stop
* Includes bowl, dough hook, whip and flat beater, all stainless steel
* See-through stainless steel safety bowl guard
* Non-slipping belt drive, provides durability for tough mixes
* Heavy duty frame with lead-free enamel coated steel for easy cleaning
* Bowl lifting by lever
* Motor overload protection
* Bowl lock automatically

Utility requirements:

* Electrical: 120V/60Hz/1Ph, 1/2 HP, 4.0 amps, NEMA 5-15P

Warranty:

* Two Years Parts and One Year Labor Warranty

Additional requirements:

* Eligible bidder must visit the installation site.
* Alternates must be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver, uncrate, set in place, level and remove crating.
* Final connections by Others.