**40-QUART PLANETARY MIXER**

Provide one (1) **40-Quart Planetary Mixer**, Model **BTF040** as manufactured by **Doyon**. Furnish with standard features as follows:

* Overall dimensions to be 23.75”W x 36” x 52.75”H
* 20 speeds – no need to stop mixer to change speeds
* Digital control with 7 programmable speed and time settings
* Emergency stop
* Includes bowl, dough hook, whip and flat beater, all stainless steel
* See-through stainless steel safety bowl guard
* Non-slipping belt drive, provides durability for tough mixes
* Heavy duty frame with lead-free enamel coated steel for easy cleaning
* 4 casters
* Bowl lifting by lever
* Motor overload protection
* Bowl lock automatically

Furnish this mixer with the following accessory features:

* Bowl Dolly

Utility requirements:

* Electrical: 208-240V/60Hz/1Ph, 3 HP, 12.0 amps, NEMA 6-15P

Warranty:

* Two Years Parts and One Year Labor Warranty

Additional requirements:

* Eligible bidder must visit the installation site.
* Alternates must be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver, uncrate, set in place, level and remove crating.
* Final connections by Others.